Instructions for Loading the SO2RDuino Software Into the K1XM SO2R Box  
   
1) Go to the  Arduino website, http://arduino.cc and  
 find the Downloads  page.  
   
2) Download and install the software for your  environment  
 (It is available for Windows, Macintosh, and  Linux).  
   
3) Download and unzip the SO2RDuino.zip file.  
   
4) Start the Arduino software and open the SO2RDuino file.  
  
5) Follow  the Arduino instructions to compile and to load  
 the firmware into  the box.